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Appendix 1 – Particular Conditions and Technical Specifications

Tender for 
Server Equipment for the Development of the GIS System at Poltava City Council





Section A:	Particular Conditions 
Section B:	Technical Specifications
1. The Buyer’s Requirements
2. The Supplier’s Technical Specifications
[bookmark: _Toc501635419]All sections which the Tenderer must complete are marked in yellow.
Section A: Particular Conditions
General background
Poltava сity сouncil established a Digitalisation Department to strengthen its capacity to develop and implement digital tools. However, the existing technical infrastructure, particularly the limited capacity of the current server equipment, poses significant challenges to the effective development and further enhancement of the city's Geographic Information System (GIS).
Recipient
Under this Agreement, the Recipient of the Goods is not the Buyer but:
Name of Recipient: Executive Committee of Poltava City Council
[bookmark: _Hlk244165877]Name of representative: Kateryna Yamschikova
[bookmark: _Hlk214525768][bookmark: _Hlk244165888][bookmark: _Hlk189655811][bookmark: _Hlk215676195]Postal address: Ukraine, Poltava, 36 Sobornosty street
Email: cancel@rada-poltava.gov.ua 
Place of delivery
The Supplier shall deliver the Goods to:
Name of location: Executive Committee of Poltava City Council 
Name of representative: Kateryna Yamschikova 
Postal address: Ukraine, Poltava, 36 Sobornosty street 
Office hours: 9:00-17:00
Time of delivery
The Supplier shall deliver the equipment and perform the scope of work no later than:
Date: 20 December 2026
Time: 17.00 Kyiv time 

Section B – Technical Specifications
1. [bookmark: _Ref516664603]The Buyer’s Requirements
The Supplier is obliged to deliver the hardware in accordance with the Buyer’s requirements and the technical specifications. In case of conflict between the Buyer’s requirements and the Supplier’s Technical Specifications, the Buyer’s Requirements shall prevail.
1.1. The tenderer must be a legally established economic operator in accordance with the legislation of its country of establishment.
1.2. The tenderer must be eligible to participate in public procurement procedures and must not be subject to any exclusion grounds as defined under applicable national public procurement legislation.
1.3. The tenderer shall demonstrate sufficient financial and economic capacity to perform the contract. Upon request, the contracting authority may require one or more of the following: annual turnover statements and/or financial statements for the last one to three financial years. The tenderer shall confirm that it has the financial stability required to ensure uninterrupted supply, warranty, and after-sales service.
1.4. The tenderer shall have proven experience in the supply of computer workstations, servers, or comparable IT hardware.
1.5. The tenderer shall demonstrate at least three (3) years of experience in supplying of comparable hardware.
1.6. The tenderer shall confirm full compliance with the minimum technical requirements specified in the Technical Specification Compliance Table.
1.7. The hardware must be manufactured in accordance with the standards, regulations, and parameters applicable in Ukraine, including DSTU[footnoteRef:1] (ISO) and TU[footnoteRef:2], approved for this type of equipment. All hardware must comply with the requirements of Ukrainian legislation applicable to this procurement item (including power supply requirements). [1:  State Standards of Ukraine (DSTU) - standards developed in accordance with the current legislation of Ukraine, which establish rules, general principles or characteristics relating to activities or their results for general and repeated application, in order to achieve an optimal degree of orderliness, developed on the basis of consensus and approved by the authorised body.]  [2:  Technical requirements (TU) that a product, process or service must meet, and defines the procedures by which it can be established whether such requirements are met. TUs set requirements for products intended for independent supply (performance, provision) and regulate the relationship between the manufacturer (supplier) and the consumer (user).] 

1.8. Any proposed equivalent equipment shall:
· meet or exceed all minimum performance parameters
· be clearly identified as equivalent
· be supported by official manufacturer documentation
1.9. The tenderer shall submit technical datasheets, certificates, or manufacturer declarations to substantiate compliance.
1.10. The Supplier certifies that in performing the services listed below, hardware or services manufactured by the following companies will not be purchased for use by the EUACI partners: Huawei Technologies Company, ZTE Corporation, Hytera Communications Corporation, Hangzhou Hikvision Digital Technology Company, and Dahua Technology Company.
1.11. All hardware supplied under the contract must be new, unused, original manufacturer products. Refurbished, reconditioned, or grey-market equipment shall not be accepted. The tenderer shall ensure traceability of equipment through serial numbers and manufacturer warranty registration.
1.12. The tenderer shall demonstrate the capability to deliver fully assembled, configured, and operational hardware.
1.13. The tenderer shall perform pre-delivery testing, including hardware diagnostics, and verification of installed components. A basic acceptance or test report shall be provided at delivery (optional).
1.14. The tenderer shall ensure that all supplied software is properly licensed, compliant with manufacturer and national licensing requirements. Proof of licensing shall be provided upon request.
1.15. The operating system shall be preinstalled prior to delivery.
1.16. The tenderer shall provide a manufacturer’s warranty period for all supplied equipment. The warranty shall cover spare parts, labour, replacement of defective components. Warranty service must be provided at no cost to the Recipient.
1.17. The tenderer shall be capable of delivering the equipment to the location specified by the contracting authority within the contractual delivery timeframe. The tenderer shall ensure appropriate packaging, protection against transport damage, compliance with handling and safety requirements.
1.18. The tenderer shall provide all required documentation. Documentation shall be provided in English and/or Ukrainian in a paper or electronic form.
1.19. The tenderer shall treat all information obtained during contract execution as confidential. The tenderer shall not access, copy, or transfer any data without prior written authorization from the contracting authority.
1.20. Final acceptance of the supplied hardware shall be subject to successful delivery, verification of compliance, acceptance testing by the beneficiary.
1.21. Failure to meet the minimum requirements may result in rejection of the tender or termination of the contract in accordance with contractual provisions.
The minimum technical requirements are provided in the table below. 



1. The Supplier’s Technical Specifications 
Tenderer must provide a completed table detailing the technical, qualitative, and quantitative characteristics of the offered hardware / software in accordance with the Buyer’s requirements. The table must include the exact specifications of the proposed hardware / software.
A server system in a 2U rackmount chassis designed for installation in a standard 19-inch server rack, intended for data processing, storage, and backup, as well as the deployment of server services and enterprise information systems.
	#
	Minimum Technical Requirement
	Offered Specification (Bidder)
	Compliance (Yes / No)
	Comments / Evidence / Datasheet Ref.

	1
	Server platform:
2U rackmount chassis, supports up to 8 hot-swappable 3.5" drives
	
	
	

	2
	Power Supply Units (PSUs):
2 redundant power supply units (PSUs) to enhance system reliability
	
	
	

	3
	CPU:
Intel Xeon 6353P, 8 cores / 8 threads, base clock frequency of 2.7 GHz, maximum Turbo frequency of up to 5.4 GHz, 24 MB cache, 95 W Thermal Design Power (TDP), LGA1700 socket.
	
	
	

	4
	RAM:
4 GB DDR5 ECC Unbuffered (2 × 32 GB), with error correction support and expandability up to 128 GB
	
	
	

	5
	System Storage Drive:
480 GB SSD, M.2 NVMe PCIe 4.0 interface, M.2 2280 form factor
	
	
	

	6
	Data Storage Drives:
2 × 4 TB HDDs, 3.5-inch form factor, SATA 6 Gb/s interface, 7,200 RPM rotational speed, Enterprise-class, Mean Time Between Failures (MTBF) of 1,200,000 hours
	
	
	

	7
	Storage Subsystem:
8 × SATA 6 Gb/s ports based on the Intel C262 chipset, with support for RAID 0, 1, 5, and 10 configurations via the integrated RAID controller
	
	
	

	8
	Network Interfaces:
2 × 1GbE RJ-45 ports based on Intel i210 controllers
	
	
	

	9
	Remote Management:
IP-KVM for remote server management, including remote console access and video output
	
	
	

	10
	Expansion Slots:
1 × PCIe x8 (in an x16 slot), 1 × PCIe x8, 2 × PCIe x4 (in x8 slots)
	
	
	

	11
	Additional Interfaces:
1 × M.2 NVMe slot, video output
	
	
	

	12
	Memory Support:
DDR5 ECC Unbuffered, 4 DIMM slots, maximum capacity of up to 128 GB
	
	
	

	13
	Operating System:
Ubuntu Linux
	
	
	



[bookmark: _Hlk214555714]


Additional Specifications and Functional Capabilities:

· Data Storage Reliability: support for RAID configurations to enhance the fault tolerance of the data storage subsystem.

· Scalability: capability for future expansion of the storage subsystem through available drive bays, as well as the installation of additional PCIe expansion cards.

· Operational Continuity: 2 power supply units providing power redundancy when connected to independent power sources or power lines.

· Ease of Maintenance: support for hot-swappable drives, allowing drive replacement without removing the server from the server rack.

· Remote Management: capability for remote diagnostics, monitoring, and server management via IP-KVM without requiring the administrator's physical presence at the equipment location.

· Energy Efficiency: use of a processor with a Thermal Design Power (TDP) of 95 W and server-grade components designed for operation in enterprise environments.

· IT Infrastructure Integration: support for standard 1 Gb/s Ethernet connectivity and installation in a standard 19-inch server rack.

· Versatility: capability to operate as a file server, application server, backup system, or platform for hosting individual virtual machines.



Signature
I, the undersigned, hereby declare that:
· I am empowered to represent the tenderer with mandate to establish a legal obligation on behalf of the tenderer in relation to the Buyer.
· I have familiarised myself with the information available to date concerning this tender procedure.
· The submitted tender is fully compliant with all requirements and that all statements, descriptions, etc. provided by the Seller in this Appendix 1 are accurately and correct.
· The statements in this Appendix 1, including attached Technical Specifications, take precedence over the Supplier’s other statements and/ or indications in the tender, if any.
· The submitted tender will be deemed to be the property of the Buyer.

	Name
	[insert name of the undersigned]

	Position
	[insert name of the undersigned]

	Date
	[insert date]

	Signature
	[insert signature]
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